**IF/ID REG (48 BITS):**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| INPUT | BITS | **47-32** | **31-16** | **15-0** |
| Signal | PC+1 | INSTRUCTION | IMM/IN |